Developer Documentation

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

All Classes Namespaces Files Functions Variables Typedefs Enumerations Enumerator Properties Friends Macros Modules Pages
Using (custom) properties

This examples shows:

- How to add and remove custom properties,
- How to get and set the value of a custom property

In the last example we computed the barycenter of each vertex' neighborhood and stored it in an array. It would be more convenient and less error-prone if we could store this data in the mesh and let OpenMesh manage the data. It would be even more helpful if we could attach such properties dynamically to the mesh.

OpenMesh provides dynamic properties, which can be attached to each mesh entity (vertex, face, edge, halfedge, and the mesh itself). We distinguish between custom and standard properties. A custom property is any user-defined property and is accessed via the member function `property`(..) via a handle and an entity handle (e.g. VertexHandle). Whereas the standard properties are accessed via special member functions, e.g. the vertex position is accessed with `point`(..) and a vertex handle.

In this example we will store the `cog-value` (see previous example) in an additional vertex property instead of keeping it in a separate array. To do so we define first a so-called property handle with the desired type (`MyMesh::Point`) and register the handle at the mesh:

// this vertex property stores the computed centers of gravity
OpenMesh::VPropHandleT<MyMesh::Point> cogs;
mesh.add_property(cogs);

The `mesh` allocates enough memory to hold as many elements of type `MyMesh::Point` as number of vertices exist, and of course the mesh synchronizes all insert and delete operations on the vertices with the vertex properties.

Once the wanted property is registered we can use the property to calculate the barycenter of the neighborhood of each vertex `v_it`

for (vv_it=mesh.vv_iter( *v_it ); vv_it; ++vv_it)
{
mesh.property(cogs,*v_it) += mesh.point( *vv_it );
++valence;
}
mesh.property(cogs,*v_it) /= valence;

and finally set the new position for each vertex `v_it`

mesh.set_point( *v_it, mesh.property(cogs,*v_it) );

Below is the complete source code:

#include <iostream>
#include <vector>
// --------------------
#include <OpenMesh/Core/IO/MeshIO.hh>
#include <OpenMesh/Core/Mesh/TriMesh_ArrayKernelT.hh>
typedef OpenMesh::TriMesh_ArrayKernelT<> MyMesh;
int main(int argc, char **argv)
{
MyMesh mesh;
// check command line options
if (argc != 4)
{
std::cerr << "Usage: " << argv[0] << " #iterations infile outfile\n";
return 1;
}
// read mesh from stdin
if ( ! OpenMesh::IO::read_mesh(mesh, argv[2]) )
{
std::cerr << "Error: Cannot read mesh from " << argv[2] << std::endl;
return 1;
}
// this vertex property stores the computed centers of gravity
OpenMesh::VPropHandleT<MyMesh::Point> cogs;
mesh.add_property(cogs);
// smoothing mesh argv[1] times
MyMesh::VertexIter v_it, v_end(mesh.vertices_end());
MyMesh::VertexVertexIter vv_it;
MyMesh::Point cog;
MyMesh::Scalar valence;
unsigned int i, N(atoi(argv[1]));
for (i=0; i < N; ++i)
{
for (v_it=mesh.vertices_begin(); v_it!=v_end; ++v_it)
{
mesh.property(cogs,*v_it).vectorize(0.0f);
valence = 0.0;
for (vv_it=mesh.vv_iter( *v_it ); vv_it; ++vv_it)
{
mesh.property(cogs,*v_it) += mesh.point( *vv_it );
++valence;
}
mesh.property(cogs,*v_it) /= valence;
}
for (v_it=mesh.vertices_begin(); v_it!=v_end; ++v_it)
if ( !mesh.is_boundary( *v_it ) )
mesh.set_point( *v_it, mesh.property(cogs,*v_it) );
}
// write mesh to stdout
if ( ! OpenMesh::IO::write_mesh(mesh, argv[3]) )
{
std::cerr << "Error: cannot write mesh to " << argv[3] << std::endl;
return 1;
}
return 0;
}