| OpenMesh

SR_types.hh
1 /* ========================================================================= *
2 * *
3 * OpenMesh *
4 * Copyright (c) 2001-2015, RWTH-Aachen University *
5 * Department of Computer Graphics and Multimedia *
6 * All rights reserved. *
7 * www.openmesh.org *
8 * *
9 *---------------------------------------------------------------------------*
10 * This file is part of OpenMesh. *
11 *---------------------------------------------------------------------------*
12 * *
13 * Redistribution and use in source and binary forms, with or without *
14 * modification, are permitted provided that the following conditions *
15 * are met: *
16 * *
17 * 1. Redistributions of source code must retain the above copyright notice, *
18 * this list of conditions and the following disclaimer. *
19 * *
20 * 2. Redistributions in binary form must reproduce the above copyright *
21 * notice, this list of conditions and the following disclaimer in the *
22 * documentation and/or other materials provided with the distribution. *
23 * *
24 * 3. Neither the name of the copyright holder nor the names of its *
25 * contributors may be used to endorse or promote products derived from *
26 * this software without specific prior written permission. *
27 * *
28 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS *
29 * "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED *
30 * TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A *
31 * PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER *
32 * OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, *
33 * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, *
34 * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR *
35 * PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF *
36 * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING *
37 * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS *
38 * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE. *
39 * *
40 * ========================================================================= */
41
42
43
44
45 //=============================================================================
46 //
47 // Helper Functions for binary reading / writing
48 //
49 //=============================================================================
50
51 #ifndef OPENMESH_SR_TYPES_HH
52 #define OPENMESH_SR_TYPES_HH
53
54
55 //== INCLUDES =================================================================
56
57 #include <OpenMesh/Core/System/config.h>
58
59
60 //== NAMESPACES ===============================================================
61
62 namespace OpenMesh {
63 namespace IO {
64
65
66 //=============================================================================
67
68
73
74 //-----------------------------------------------------------------------------
75
76 typedef unsigned char uchar;
77 typedef unsigned short ushort;
78 typedef unsigned long ulong;
79
80 typedef signed char int8_t; typedef unsigned char uint8_t;
81 typedef short int16_t; typedef unsigned short uint16_t;
82
83 // Int should be 32 bit on all archs.
84 // long is 32 under windows but 64 under unix 64 bit
85 typedef int int32_t; typedef unsigned int uint32_t;
86 #if defined(OM_CC_MSVC)
87 typedef __int64 int64_t; typedef unsigned __int64 uint64_t;
88 #else
89 typedef long long int64_t; typedef unsigned long long uint64_t;
90 #endif
91
92 typedef float float32_t;
93 typedef double float64_t;
94
95 typedef uint8_t rgb_t[3];
96 typedef uint8_t rgba_t[4];
97
99
100
101 //=============================================================================
102 } // namespace IO
103 } // namespace OpenMesh
104 //=============================================================================
105 #endif // OPENMESH_MESHREADER_HH defined
106 //=============================================================================
107
OpenMesh::IO::ulong
unsigned long ulong
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:78
OpenMesh::IO::rgb_t
uint8_t rgb_t[3]
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:95
OpenMesh::IO::float64_t
double float64_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:93
OpenMesh::IO::int16_t
short int16_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:81
OpenMesh::IO::ushort
unsigned short ushort
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:77
OpenMesh::IO::int32_t
int int32_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:85
OpenMesh::IO::float32_t
float float32_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:92
OpenMesh::IO::uint8_t
unsigned char uint8_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:80
OpenMesh::IO::uint32_t
unsigned int uint32_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:85
OpenMesh::IO::rgba_t
uint8_t rgba_t[4]
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:96
OpenMesh
Contains all the mesh ingredients like the polygonal mesh, the triangle mesh, different mesh kernels ...
Definition: MeshItems.hh:59
OpenMesh::IO::uint64_t
unsigned long long uint64_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:89
OpenMesh::IO::int64_t
long long int64_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:89
OpenMesh::IO::uchar
unsigned char uchar
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:76
OpenMesh::IO::uint16_t
unsigned short uint16_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:81
OpenMesh::IO::int8_t
signed char int8_t
Binary read a short from _is and perform byte swapping if _swap is true.
Definition: SR_types.hh:80